# University Health and Safety Form

# ROUTINE Radiation SURVEY

The following information is required upon the installation or movement of any equipment that is used to generate Ionising Radiation. This information is required by Regulation 32(2) of the Ionising Radiation Regulations 2017.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1. SURVEY INFORMATION** | | | | | |
| **Date of Survey** | **Time of Survey** | **Building** | **Room No.** | **Department** | **Survey Reference** |
|  |  |  |  |  |  |
| **Monitor / Counter Used** | **Monitor / Counter Serial No.** | **Monitor Calibration date** | **Background Reading** | | |
|  |  | |  | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1. EXAMINATION SURVEY** | | | | | |
|  | **Description of Point** | **Dose Recorded** |  | **Description of Point** | **Dose Recorded** |
| **Point 1** |  | **uSv / hr** | **Point 11** |  | **uSv / hr** |
| **Point 2** |  | **uSv / hr** | **Point 12** |  | **uSv / hr** |
| **Point 3** |  | **uSv / hr** | **Point 13** |  | **uSv / hr** |
| **Point 4** |  | **uSv / hr** | **Point 14** |  | **uSv / hr** |
| **Point 5** |  | **uSv / hr** | **Point 15** |  | **uSv / hr** |
| **Point 6** |  | **uSv / hr** | **Point 16** |  | **uSv / hr** |
| **Point 7** |  | **uSv / hr** | **Point 17** |  | **uSv / hr** |
| **Point 8** |  | **uSv / hr** | **Point 18** |  | **uSv / hr** |
| **Point 9** |  | **uSv / hr** | **Point 19** |  | **uSv / hr** |
| **Point 10** |  | **uSv / hr** | **Point 20** |  | **uSv / hr** |

Should the reading at any location be more than 5uSv / hr than the previous reading at this location, the point is to be surveyed again. If the elevated readings continue, the University Radiation Protection Officer (URPO) is to be contacted immediately.

**Ensure that a suitable diagram is attached, showing all noted survey points.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **3. ADMINISTRATIVE INFORMATION** | | | | | |
| **Survey Completed by** | | | | | |
| **Name:** |  | **Signature:** |  | **Date:** |  |